{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":78,"n_cols":7,"rows_kept":78,"cut":false,"hidden":false,"merged":[]}
["变量名(英文)","类型","中文释义","读写方式","地址"]
["f1fAxleTempFront  ","Float","1#1级前轴温","只读",{"$f":"\"x=3;\"&TEXT(G2, \"0000\")","v":"x=3;0001"},null,1]
["f1fAxleTempRear  ","Float","1#1级后轴温","只读",{"$f":"\"x=3;\"&TEXT(G3, \"0000\")","v":"x=3;0003"},null,{"$f":"G2+2","v":3}]
["f1fStatorTemp1  ","Float","1#1级定子温度1","只读","x=3;0005",null,{"$f":"G3+2","v":5}]
["f1fStatorTemp2  ","Float","1#1级定子温度2","只读","x=3;0007",null,7]
["f1fStatorTemp3  ","Float","1#1级定子温度3","只读","x=3;0009",null,9]
["f2fAxleTempFront  ","Float","1#2级前轴温","只读","x=3;0011",null,11]
["f2fAxleTempRear  ","Float","1#2级后轴温","只读","x=3;0013",null,13]
["f2fStatorTemp1  ","Float","1#2级定子温度1","只读","x=3;0015",null,15]
["f2fStatorTemp2  ","Float","1#2级定子温度2","只读","x=3;0017",null,17]
["f2fStatorTemp3  ","Float","1#2级定子温度3","只读","x=3;0019",null,19]
["s1fAxleTempFront  ","Float","2#1级前轴温","只读","x=3;0021",null,{"$f":"G11+2","v":21}]
["s1fAxleTempRear  ","Float","2#1级后轴温","只读","x=3;0023",null,23]
["s1fStatorTemp1  ","Float","2#1级定子温度1","只读","x=3;0025",null,25]
["s1fStatorTemp2  ","Float","2#1级定子温度2","只读","x=3;0027",null,{"$f":"G14+2","v":27}]
["s1fStatorTemp3  ","Float","2#1级定子温度3","只读","x=3;0029",null,29]
["s2fAxleTempFront  ","Float","2#2级前轴温","只读","x=3;0031",null,31]
["s2fAxleTempRear  ","Float","2#2级后轴温","只读","x=3;0033",null,33]
["s2fStatorTemp1  ","Float","2#2级定子温度1","只读","x=3;0035",null,35]
["s2fStatorTemp2  ","Float","2#2级定子温度2","只读","x=3;0037",null,37]
["s2fStatorTemp3  ","Float","2#2级定子温度3","只读","x=3;0039",null,39]
["f1fOutputV  ","Float","1#1级输出电压","只读","x=3;0041",null,41]
["f1fOutputC  ","Float","1#1级输出电流","只读","x=3;0043",null,43]
["f1fOutputP  ","Float","1#1级输出功率","只读","x=3;0045",null,45]
["f1fFreq  ","Float","1#1级运行频率","只读","x=3;0047",null,47]
["f2fOutputV  ","Float","1#2级输出电压","只读","x=3;0049",null,49]
["f2fOutputC  ","Float","1#2级输出电流","只读","x=3;0051",null,51]
["f2fOutputP  ","Float","1#2级输出功率","只读","x=3;0053",null,53]
["f2fFreq  ","Float","1#2级运行频率","只读","x=3;0055",null,55]
["s1fOutputV  ","Float","2#1级输出电压","只读","x=3;0057",null,57]
["s1fOutputC  ","Float","2#1级输出电流","只读","x=3;0059",null,59]
["s1fOutputP  ","Float","2#1级输出功率","只读","x=3;0061",null,61]
["s1fFreq  ","Float","2#1级运行频率","只读","x=3;0063",null,63]
["s2fOutputV  ","Float","2#2级输出电压","只读","x=3;0065",null,65]
["s2fOutputC  ","Float","2#2级输出电流","只读","x=3;0067",null,67]
["s2fOutputP  ","Float","2#2级输出功率","只读","x=3;0069",null,69]
["s2fFreq  ","Short","2#2级运行频率","只读","x=3;0071",null,71]
["f1SP  ","Float","1#风机静压","只读","x=3;0073",null,73]
["f1TP  ","Float","1#风机全压","只读","x=3;0075",null,75]
["f1AF  ","Float","1#风机风量","只读","x=3;0077",null,77]
["f1AS  ","Float","1#风机风速","只读","x=3;0079",null,79]
["f1E  ","Float","1#风机效率","只读","x=3;0081",null,81]
["f1H1Vib  ","Float","1#1机水平振动","只读","x=3;0083",null,83]
["f11VVib  ","Float","1#1级垂直振动","只读","x=3;0085",null,85]
["f1H2Vib  ","Float","1#2机水平振动","只读","x=3;0087",null,87]
["f12VVib  ","Float","1#2级垂直振动","只读","x=3;0089",null,89]
["f2SP  ","Float","2#风机静压","只读","x=3;0091",null,91]
["f2TP  ","Float","2#风机全压","只读","x=3;0093",null,93]
["f2AF  ","Float","2#风机风量","只读","x=3;0095",null,95]
["f2AS  ","Float","2#风机风速","只读","x=3;0097",null,{"$f":"G49+2","v":97}]
["f2E  ","Short","2#风机效率","只读","x=3;0099",null,99]
["f2H1Vib  ","Float","2#1机水平振动","只读","x=3;0101",null,101]
["f21VVib  ","Float","2#1级垂直振动","只读","x=3;0103",null,103]
["f2H2Vib  ","Float","2#2机水平振动","只读","x=3;0105",null,105]
["f22VVib  ","Float","2#2级垂直振动","只读","x=3;0107",null,107]
["lrMode  ","Boolean","就地远程","只读",{"$f":"\"x=1;\"&TEXT(G56, \"0000\")","v":"x=1;0001"},null,1]
["f1ISStatus  ","Boolean","1#进线合分闸状态","只读",{"$f":"\"x=1;\"&TEXT(G57, \"0000\")","v":"x=1;0002"},null,2]
["f2ISStatus  ","Boolean","2#进线合分闸状态","只读","x=1;0003",null,3]
["f1HDOpen  ","Boolean","1#水平风门开到位","只读","x=1;0004",null,4]
["f1HDClose  ","Boolean","1#水平风门关到位","只读","x=1;0005",null,5]
["f1VDOpen  ","Boolean","1#竖风门开到位","只读","x=1;0006",null,6]
["f1VDClose  ","Boolean","1#竖风门关到位","只读","x=1;0007",null,7]
["f1MDOpen  ","Boolean","1#检修风门开到位","只读","x=1;0008",null,8]
["f1MDClose  ","Boolean","1#检修风门关到位","只读","x=1;0009",null,9]
["f2HDOpen  ","Boolean","2#水平风门开到位","只读","x=1;0010",null,10]
["f2HDClose  ","Boolean","2#水平风门关到位","只读","x=1;0011",null,11]
["f2VDOpen  ","Boolean","2#竖风门开到位","只读","x=1;0012",null,12]
["f2VDClose  ","Boolean","2#竖风门关到位","只读","x=1;0013",null,13]
["f2MDOpen  ","Boolean","2#检修风门开到位","只读","x=1;0014",null,14]
["f2MDClose  ","Boolean","2#检修风门关到位","只读","x=1;0015",null,15]
["f11RunStatus  ","Boolean","1#1级运行状态","只读","x=1;0016",null,16]
["f11FaultStatus  ","Boolean","1#1级故障状态","只读","x=1;0017",null,17]
["f12RunStatus  ","Boolean","1#2级运行状态","只读","x=1;0018",null,18]
["f12FaultStatus  ","Boolean","1#2级故障状态","只读","x=1;0019",null,19]
["s21RunStatus  ","Boolean","2#1级运行状态","只读","x=1;0020",null,20]
["s21FaultStatus  ","Boolean","2#1级故障状态","只读","x=1;0021",null,21]
["s22RunStatus  ","Boolean","2#2级运行状态","只读","x=1;0022",null,22]
["s22FaultStatus","Boolean","2#2级故障状态","只读","x=1;0023",null,23]