{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":147,"n_cols":5,"rows_kept":147,"cut":false,"hidden":false,"merged":[]}
["变量名(英文)","类型","中文释义","读写方式","地址"]
["inletSelection  ","Short","进线选择","读写","MW2376"]
["opRunTime1  ","Float","一号本次运行时间","读写","MD608"]
["mode  ","Short","方式","读写","MW2380"]
["startCountdown1  ","Short","一号启动倒计时","只读","MW3012"]
["freqRunCurrent1_1","Short","一号变频运行电流1","只读","MW1116"]
["alarmDelay  ","Float","报警延时","读写","MD2360"]
["accRunTime1Level1  ","Float","一号一级累计运行时间","读写","MD600"]
["shaftTempAlarm  ","Float","轴温报警值","读写","MD2364"]
["fixedTempAlarm  ","Float","定温报警值","读写","MD2368"]
["vibCoeff1Level1Horz  ","Float","一号一级水平振动系数","读写","MD2276"]
["vibCoeff1Level1Vert  ","Float","一号一级垂直振动系数","读写","MD2280"]
["vibCoeff1Level2Horz  ","Float","一号二级水平振动系数","读写","MD2284"]
["staticPressureCoeff1  ","Float","一号静压系数","读写","MD2292"]
["totalPressureCoeff1  ","Float","一号全压系数","读写","MD2296"]
["vibCoeff1Level2Vert  ","Float","一号二级垂直振动系数","读写","MD2288"]
["tempCoeff1Level1Front  ","Float","一号一级前轴温度系数","读写","MD2300"]
["tempCoeff1Level1Rear  ","Float","一号一级后轴温度系数","读写","MD2232"]
["tempCoeff1Level1Fixed1  ","Float","一号一级定温1系数","读写","MD2304"]
["tempCoeff1Level1Fixed2  ","Float","一号一级定温2系数","读写","MD2308"]
["tempCoeff1Level2Front  ","Float","一号二级前轴温度系数","读写","MD2312"]
["tempCoeff1Level2Rear  ","Float","一号二级后轴温度系数","读写","MD2316"]
["tempCoeff1Level2Fixed1  ","Float","一号二级定温1系数","读写","MD2320"]
["tempCoeff1Level2Fixed2  ","Float","一号二级定温2系数","读写","MD2324"]
["voltageRatio  ","Float","电压变比","读写","MD2352"]
["currentRatio  ","Float","电流变比","读写","MD2356"]
["fanModel  ","Float","风机型号","读写","MD2384"]
["resistanceLoss  ","Float","阻力损耗","读写","MD2388"]
["windSpeedCoeff1  ","Float","一号风速系数","读写","MD2344"]
["fanEfficiencyCoeff1  ","Float","一号风机效率系数","读写","MD2328"]
["vibrationAlarmValue  ","Float","振动报警值","读写","MD2372"]
["airFlowCoeff1  ","Float","一号风量系数","读写","MD2332"]
["rpmPlc1  ","Float","一号转速plc","读写","MD2348"]
["inletCurrentRatio  ","Float","进线电流变比","读写","MD2396"]
["bladeAngle1  ","Float","一号风叶角度","读写","MD2400"]
["bladeAngle2  ","Float","二号风叶角度","读写","MD2404"]
["lowVoltageAlarm  ","Float","低压报警值","读写","MD2408"]
["inletCurrentPlc1  ","Float","一号进线电流plc","读写","MD2412"]
["currentBPlc1_1  ","Float","一号一电流Bplc","读写","MD2416"]
["currentCPlc1_1  ","Float","一号一电流Cplc","读写","MD2420"]
["currentBPlc1_2  ","Float","一号二电流Bplc","读写","MD2424"]
["currentCPlc1_2  ","Float","一号二电流Cplc","读写","MD2428"]
["freqRunCurrent1  ","Short","一号变频运行电流1","只读","MW1116"]
["runFreq1_1  ","Float","一号一运行频率","只读","MW1100"]
["freqGiven1_1  ","Float","一号一频率给定","读写","MD1108"]
["hubRatio  ","Float","轮毂比","读写","MD2392"]
["tempCoeff1Level1Fixed3  ","Float","一号一级定温3系数","读写","MD2336"]
["tempCoeff1Level2Fixed3  ","Float","一号二级定温3系数","读写","MD2340"]
["tempPlc1Level1Fixed3  ","Float","一号一级定温3plc","读写","MD2180"]
["tempPlc1Level2Fixed3  ","Float","一号二级定温3plc","读写","MD2184"]
["totalPressurePlc1  ","Float","一号全压plc","读写","MD2064"]
["vibPlc1Level1Horz  ","Float","一号一级水平振动plc","读写","MD2028"]
["vibPlc1Level2Horz  ","Float","一号二级水平振动plc","读写","MD2060"]
["staticPressurePlc1  ","Float","一号静压plc","读写","MD2072"]
["vibPlc1Level1Vert  ","Float","一号一级垂直振动plc","读写","MD2016"]
["vibPlc1Level2Vert  ","Float","一号二级垂直振动plc","读写","MD2048"]
["voltagePlc1  ","Float","一号电压plc","读写","MD2176"]
["currentPlc1_1  ","Float","一号一电流plc","读写","MD2004"]
["airFlowPlc1  ","Float","一号风量plc","读写","MD2084"]
["tempPlc1Level1Front  ","Float","一号一级前轴温度plc","读写","MD2008"]
["tempPlc1Level1Rear  ","Float","一号一级后轴温度plc","读写","MD2012"]
["tempPlc1Level1Fixed1  ","Float","一号一级定温1plc","读写","MD2020"]
["tempPlc1Level1Fixed2  ","Float","一号一级定温2plc","读写","MD2024"]
["tempPlc1Level2Front  ","Float","一号二级前轴温度plc","读写","MD2040"]
["tempPlc1Level2Rear  ","Float","一号二级后轴温度plc","读写","MD2044"]
["tempPlc1Level2Fixed1  ","Float","一号二级定温1plc","读写","MD2052"]
["tempPlc1Level2Fixed2  ","Float","一号二级定温2plc","读写","MD2056"]
["fanEfficiencyPlc1  ","Float","一号风机效率plc","读写","MD2076"]
["currentPlc1_2  ","Float","一号二电流plc","读写","MD2036"]
["fanSpeedPlc1  ","Float","一号风机风速plc","读写","MD2080"]
["powerPlc1_2  ","Float","一号二功率plc","读写","MD2032"]
["powerPlc1_1  ","Float","一号一功率plc","读写","MD2000"]
["vibError1Level1Horz  ","Float","一号一级水平振动误差","读写","MD2196"]
["vibError1Level1Vert  ","Float","一号一级垂直振动误差","读写","MD2200"]
["vibError1Level2Horz  ","Float","一号二级水平振动误差","读写","MD2204"]
["staticPressureError1  ","Float","一号静压误差","读写","MD2208"]
["totalPressureError1  ","Float","一号全压误差","读写","MD2212"]
["vibError1Level2Vert  ","Float","一号二级垂直振动误差","读写","MD2216"]
["tempError1Level1Front  ","Float","一号一级前轴温度误差","读写","MD2220"]
["tempError1Level1Rear  ","Float","一号一级后轴温度误差","读写","MD2224"]
["tempError1Level1Fixed1  ","Float","一号一级定温1误差","读写","MD2228"]
["tempError1Level1Fixed2  ","Float","一号一级定温2误差","读写","MD2236"]
["tempError1Level2Front  ","Float","一号二级前轴温度误差","读写","MD2240"]
["tempError1Level2Rear  ","Float","一号二级后轴温度误差","读写","MD2244"]
["tempError1Level2Fixed1  ","Float","一号二级定温1误差","读写","MD2248"]
["tempError1Level2Fixed2  ","Float","一号二级定温2误差","读写","MD2252"]
["windSpeedError1  ","Float","一号风速误差","读写","MD2256"]
["fanEfficiencyError1  ","Float","一号风机效率误差","读写","MD2260"]
["airFlowError1  ","Float","一号风量误差","读写","MD2264"]
["tempError1Level1Fixed3  ","Float","一号一级定温3误差","读写","MD2268"]
["tempError1Level2Fixed3  ","Float","一号二级定温3误差","读写","MD2272"]
["horzDoorOpen1  ","Float","一号水平门开度","只读","MD1104"]
["baffleDoorOpen1  ","Float","一号挡板门开度","只读","MD1112"]
["butterValveOpen1  ","Boolean","一号蝶阀开","读写","M1.7"]
["butterValveClose1  ","Boolean","一号蝶阀关","读写","M2.0"]
["butterValveStop1  ","Boolean","一号蝶阀停","读写","M2.1"]
["butterValveOpenPos1  ","Boolean","一号蝶阀开到位","只读","I1.6"]
["butterValveClosePos1  ","Boolean","一号蝶阀关到位","只读","I1.7"]
["transformerOutputClose1  ","Boolean","一号变压器出线合闸","只写","M0.2"]
["brake1Level1  ","Boolean","一号一级刹车","读写","M3.3"]
["transformerOutputOpen1  ","Boolean","一号变压器出线分闸","只写","M0.3"]
["singleMotor1Close  ","Boolean","单电机1合闸","只写","M0.4"]
["singleMotor1Open  ","Boolean","单电机1分闸","只写","M0.5"]
["inletCloseIndic1  ","Boolean","一号进线合闸指示","只读","I0.1"]
["tieCloseIndic  ","Boolean","联络合闸指示","只读","I2.4"]
["alarmSoundOutput  ","Boolean","报警声音输出","读写","M2.7"]
["inletClose1  ","Boolean","一号进线合闸","读写","M0.0"]
["inletOpen1  ","Boolean","一号进线分闸","读写","M0.1"]
["brakeRelease1Level1  ","Boolean","一号一级松刹车","读写","M3.4"]
["brake1Level2  ","Boolean","一号二级刹车","读写","M3.5"]
["brakeRelease1Level2  ","Boolean","一号二级松刹车","读写","M3.6"]
["pressureAlarmBtn  ","Boolean","风压报警按钮","读写","M2500.0"]
["tieClose  ","Boolean","联络合闸","读写","M2.5"]
["tieOpen  ","Boolean","联络分闸","读写","M2.6"]
["lock1  ","Boolean","闭锁1","读写","M700.0"]
["horzDoorOpenPos1  ","Boolean","一号水平门开到位","只读","I2.2"]
["horzDoorClosePos1  ","Boolean","一号水平门关到位","只读","I2.1"]
["vertDoorOpenPos1  ","Boolean","一号垂直门开到位","只读","I2.6"]
["vertDoorClosePos1  ","Boolean","一号垂直门关到位","只读","I2.7"]
["horzDoorToOpen1  ","Boolean","一号水平门开","读写","M2.2"]
["horzDoorStop1  ","Boolean","一号水平门停","读写","M2.4"]
["horzDoorClose1  ","Boolean","一号水平门关","读写","M2.3"]
["vertDoorOpen1  ","Boolean","一号垂直门开","读写","M3.0"]
["vertDoorStop1  ","Boolean","一号垂直门停","读写","M3.2"]
["vertDoorClose1  ","Boolean","一号垂直门关","读写","M3.1"]
["singleMotor2Close  ","Boolean","单电机2合闸","只写","M0.6"]
["singleMotor2Open  ","Boolean","单电机2分闸","只写","M0.7"]
["feedClose1  ","Boolean","一号馈电合闸","只写","M1.0"]
["feedOpen1  ","Boolean","一号馈电分闸","只写","M1.1"]
["inverterReverseStart1  ","Boolean","一号变频器反转启动","只写","M1.3"]
["inverterForwardStart1  ","Boolean","一号变频器正转启动","只写","M1.2"]
["inverterStop1  ","Boolean","一号变频器停止","只写","M1.4"]
["inverterReset1  ","Boolean","一号变频器复位","只写","M1.5"]
["inletRemote1  ","Boolean","一号进线远程","只读","I0.0"]
["transformerRemote1  ","Boolean","一号变压器远程","只读","I0.2"]
["singleMotorCabinetRemote1  ","Boolean","一号单电机柜远程","只读","I0.4"]
["horzDoorRemote1  ","Boolean","一号水平门远程","只读","I2.0"]
["tieRemote  ","Boolean","联络远程","只读","I2.3"]
["vertDoorRemote1  ","Boolean","一号垂直门远程","只读","I2.5"]
["transformerOutputStatus1  ","Boolean","一号变压器出线状态","只读","I0.3"]
["singleMotor1Status1  ","Boolean","一号单电机1状态","只读","I0.5"]
["singleMotor2Status1  ","Boolean","一号单电机2状态","只读","I0.6"]
["feedRemoteIndic1  ","Boolean","一号馈电远程指示","只读","I0.7"]
["feedRunIndic1  ","Boolean","一号馈电运行指示","只读","I1.0"]
["inverterRunIndic1  ","Boolean","一号变频器正运行指示","只读","I1.4"]
["inverterFault1  ","Boolean","一号变频器故障","只读","I1.3"]
["inverterReverseIndic1","Boolean","一号变频器反运行指示","只读","I1.5"]