{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":130,"n_cols":5,"rows_kept":130,"cut":false,"hidden":false,"merged":[]}
["变量名(英文)","类型","中文释义","读写方式","地址"]
["inputSelection  ","Short","进线选择","读写","MW2376"]
["startupCountdown2  ","UShort","二号启动倒计时","只读","MW3012"]
["runTimeCurrent2  ","Float","二号本次运行时间","读写","MD608"]
["frequencyCurrent1_2  ","Short","二号变频运行电流1","只读","MW1116"]
["cumulativeRunTime1Level2  ","Float","二号一级累计运行时间","读写","MD600"]
["voltagePLC2  ","Float","二号电压plc","读写","MD2068"]
["vibrationCoeffHorizontal1Level2  ","Float","二号一级水平振动系数","读写","MD2344"]
["vibrationCoeffVertical1Level2  ","Float","二号一级垂直振动系数","读写","MD2340"]
["vibrationCoeffHorizontal2Level2  ","Float","二号二级水平振动系数","读写","MD2336"]
["vibrationCoeffVertical2Level2  ","Float","二号二级垂直振动系数","读写","MD2332"]
["tempCoeffFrontAxle1Level2  ","Float","二号一级前轴温度系数","读写","MD2328"]
["tempCoeffRearAxle1Level2  ","Float","二号一级后轴温度系数","读写","MD2324"]
["tempCoeffFixed1_2  ","Float","二号一级定温1系数","读写","MD2320"]
["staticPressureCoeff2  ","Float","二号静压系数","读写","MD2316"]
["totalPressureCoeff2  ","Float","二号全压系数","读写","MD2312"]
["tempCoeffFixed2_2  ","Float","二号一级定温2系数","读写","MD2308"]
["tempCoeffFrontAxle2Level2  ","Float","二号二级前轴温度系数","读写","MD2304"]
["tempCoeffRearAxle2Level2  ","Float","二号二级后轴温度系数","读写","MD2300"]
["tempCoeffFixed1_3  ","Float","二号二级定温1系数","读写","MD2296"]
["tempCoeffFixed2_3  ","Float","二号二级定温2系数","读写","MD2292"]
["windSpeedCoeff2  ","Float","二号风速系数","读写","MD2288"]
["fanEfficiencyCoeff2  ","Float","二号风机效率系数","读写","MD2284"]
["airflowCoeff2  ","Float","二号风量系数","读写","MD2280"]
["speedPLC2  ","Float","二号转速plc","读写","MD2348"]
["inputCurrentPLC2  ","Float","二号进线电流plc","读写","MD2412"]
["currentBPLC2_1  ","Float","二号一电流Bplc","读写","MD2416"]
["currentCPLC2_1  ","Float","二号一电流Cplc","读写","MD2420"]
["currentBPLC2_2  ","Float","二号二电流Bplc","读写","MD2424"]
["currentCPLC2_2  ","Float","二号二电流Cplc","读写","MD2428"]
["frequencyCurrent2  ","Short","二号变频运行电流","只读","MW1116"]
["runFrequency2_1  ","Float","二号一运行频率","只读","MD1100"]
["frequencyGiven2_1  ","Float","二号一频率给定","读写","MD1108"]
["tempCoeffFixed3_2Level2  ","Float","二号二级定温3系数","读写","MD2276"]
["tempCoeffFixed3_1Level2  ","Float","二号一级定温3系数","读写","MD2272"]
["tempFixed3PLC1Level2  ","Float","二号一级定温3plc","读写","MD2188"]
["tempFixed3PLC2Level2  ","Float","二号二级定温3plc","读写","MD2192"]
["vibrationCoeffHorizontalPLC2Level2  ","Float","二号二级水平振动plc","读写","MD2172"]
["staticPressurePLC2  ","Float","二号静压plc","读写","MD2156"]
["vibrationCoeffHorizontalPLC1Level2  ","Float","二号一级水平振动plc","读写","MD2116"]
["vibrationCoeffVerticalPLC1Level2  ","Float","二号一级垂直振动plc","读写","MD2104"]
["vibrationCoeffVerticalPLC2Level2  ","Float","二号二级垂直振动plc","读写","MD2136"]
["powerPLC2_1  ","Float","二号一功率plc","读写","MD2088"]
["airflowPLC2  ","Float","二号风量plc","读写","MD2168"]
["tempRearAxlePLC1Level2  ","Float","二号一级后轴温度plc","读写","MD2100"]
["tempFrontAxlePLC1Level2  ","Float","二号一级前轴温度plc","读写","MD2096"]
["tempFixed1PLC1Level2  ","Float","二号一级定温1plc","读写","MD2108"]
["tempFixed2PLC1Level2  ","Float","二号一级定温2plc","读写","MD2112"]
["tempFrontAxlePLC2Level2  ","Float","二号二级前轴温度plc","读写","MD2128"]
["tempRearAxlePLC2Level2  ","Float","二号二级后轴温度plc","读写","MD2132"]
["tempFixed1PLC2Level2  ","Float","二号二级定温1plc","读写","MD2140"]
["tempFixed2PLC2Level2  ","Float","二号二级定温2plc","读写","MD2144"]
["totalPressurePLC2  ","Float","二号全压plc","读写","MD2152"]
["fanEfficiencyPLC2  ","Float","二号风机效率plc","读写","MD2160"]
["fanSpeedPLC2  ","Float","二号风机风速plc","读写","MD2164"]
["currentPLC2_2  ","Float","二号二电流plc","读写","MD2124"]
["powerPLC2_2  ","Float","二号二功率plc","读写","MD2120"]
["currentPLC2_1  ","Float","二号一电流plc","读写","MD2092"]
["vibrationErrorHorizontal1Level2  ","Float","二号一级水平振动误差","读写","MD2196"]
["vibrationErrorVertical1Level2  ","Float","二号一级垂直振动误差","读写","MD2200"]
["vibrationErrorHorizontal2Level2  ","Float","二号二级水平振动误差","读写","MD2204"]
["vibrationErrorVertical2Level2  ","Float","二号二级垂直振动误差","读写","MD2208"]
["tempErrorFrontAxle1Level2  ","Float","二号一级前轴温度误差","读写","MD2212"]
["tempErrorRearAxle1Level2  ","Float","二号一级后轴温度误差","读写","MD2216"]
["tempErrorFixed1_2  ","Float","二号一级定温1误差","读写","MD2220"]
["tempErrorFixed2_2  ","Float","二号一级定温2误差","读写","MD2224"]
["tempErrorFrontAxle2Level2  ","Float","二号二级前轴温度误差","读写","MD2228"]
["tempErrorRearAxle2Level2  ","Float","二号二级后轴温度误差","读写","MD2232"]
["tempErrorFixed1_3  ","Float","二号二级定温1误差","读写","MD2236"]
["tempErrorFixed2_3  ","Float","二号二级定温2误差","读写","MD2240"]
["windSpeedError2  ","Float","二号风速误差","读写","MD2244"]
["fanEfficiencyError2  ","Float","二号风机效率误差","读写","MD2248"]
["airflowError2  ","Float","二号风量误差","读写","MD2252"]
["tempErrorFixed3_2  ","Float","二号二级定温3误差","读写","MD2256"]
["tempErrorFixed3_1  ","Float","二号一级定温3误差","读写","MD2260"]
["staticPressureError2  ","Float","二号静压误差","读写","MD2264"]
["totalPressureError2  ","Float","二号全压误差","读写","MD2268"]
["horizontalDoorOpenDegree2  ","Float","二号水平门开度","只读","MD1112"]
["baffleDoorOpenDegree2  ","Float","二号挡板门开度","只读","MD1104"]
["butterValveOpen2  ","Boolean","二号蝶阀开","读写","M1.7"]
["butterValveClose2  ","Boolean","二号蝶阀关","读写","M2.0"]
["butterValveStop2  ","Boolean","二号蝶阀停","读写","M2.1"]
["butterValveOpenLimit2  ","Boolean","二号蝶阀开到位","只读","I1.6"]
["butterValveCloseLimit2  ","Boolean","二号蝶阀关到位","只读","I1.7"]
["inputLineCloseIndication2  ","Boolean","二号进线合闸指示","只读","I0.1"]
["inputLineClose2  ","Boolean","二号进线合闸","只写","M0.0"]
["inputLineOpen2  ","Boolean","二号进线分闸","只写","M0.1"]
["brake1Level2  ","Boolean","二号一级刹车","读写","M3.3"]
["brakeRelease1Level2  ","Boolean","二号一级松刹车","读写","M3.4"]
["brake2Level2  ","Boolean","二号二级刹车","读写","M3.5"]
["brakeRelease2Level2  ","Boolean","二号二级松刹车","读写","M3.6"]
["lock  ","Boolean","闭锁","读写","M700.0"]
["upsPower1  ","Boolean","ups1路电源","读写","I3.6"]
["upsPower2  ","Boolean","ups2路电源","读写","I3.7"]
["horizontalDoorOpenLimit2  ","Boolean","二号水平门开到位","只读","I2.6"]
["horizontalDoorCloseLimit2  ","Boolean","二号水平门关到位","只读","I2.7"]
["verticalDoorOpenLimit2  ","Boolean","二号垂直门开到位","只读","I2.1"]
["verticalDoorCloseLimit2  ","Boolean","二号垂直门关到位","只读","I2.2"]
["horizontalDoorOpen2  ","Boolean","二号水平门开","读写","M3.0"]
["horizontalDoorStop2  ","Boolean","二号水平门停","读写","M3.2"]
["horizontalDoorClose2  ","Boolean","二号水平门关","读写","M3.1"]
["verticalDoorOpen2  ","Boolean","二号垂直门开","读写","M2.2"]
["verticalDoorStop2  ","Boolean","二号垂直门停","读写","M2.4"]
["verticalDoorClose2  ","Boolean","二号垂直门关","读写","M2.3"]
["transformerLineClose2  ","Boolean","二号变压器出线合闸","只写","M0.2"]
["transformerLineOpen2  ","Boolean","二号变压器出线分闸","只写","M0.3"]
["singleMotor1Close2  ","Boolean","二号单电机1合闸","只写","M0.4"]
["singleMotor1Open2  ","Boolean","二号单电机1分闸","只写","M0.5"]
["singleMotor2Close2  ","Boolean","二号单电机2合闸","只写","M0.6"]
["singleMotor2Open2  ","Boolean","二号单电机2分闸","只写","M0.7"]
["feederClose2  ","Boolean","二号馈电合闸","只写","M1.0"]
["feederOpen2  ","Boolean","二号馈电分闸","只写","M1.1"]
["inverterReverseStart2  ","Boolean","二号变频器反转启动","只写","M1.3"]
["inverterForwardStart2  ","Boolean","二号变频器正转启动","只写","M1.2"]
["inverterStop2  ","Boolean","二号变频器停止","只写","M1.4"]
["inverterReset2  ","Boolean","二号变频器复位","只写","M1.5"]
["inputLineRemote2  ","Boolean","二号进线远程","只读","I0.0"]
["transformerRemote2  ","Boolean","二号变压器远程","只读","I0.2"]
["singleMotorCabinetRemote2  ","Boolean","二号单电机柜远程","只读","I0.4"]
["horizontalDoorRemote2  ","Boolean","二号水平门远程","只读","I2.5"]
["verticalDoorRemote2  ","Boolean","二号垂直门远程","只读","I2.0"]
["transformerLineStatus2  ","Boolean","二号变压器出线状态","只读","I0.3"]
["singleMotor1Status2  ","Boolean","二号单电机1状态","只读","I0.5"]
["singleMotor2Status2  ","Boolean","二号单电机2状态","只读","I0.6"]
["feederRunningIndication2  ","Boolean","二号馈电运行指示","只读","I1.0"]
["inverterRunningIndication2  ","Boolean","二号变频器正运行指示","只读","I1.4"]
["inverterFault2  ","Boolean","二号变频器故障","只读","I1.3"]
["inverterReverseRunningIndication2  ","Boolean","二号变频器反运行指示","只读","I1.5"]
["feederRemote2  ","Boolean","二号馈电远程","读写","I0.7"]
["failoverSwitch","Boolean","故障切换开关","读写","M10.0"]