{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":107,"n_cols":5,"rows_kept":107,"cut":false,"hidden":false,"merged":[]}
["变量名(英文)","类型","中文释义","读写方式","地址"]
["f1Uab","Float","F1_Uab","只读","DB100.0"]
["f1Ubc","Float","F1_Ubc","只读","DB100.4"]
["f1Uca","Float","F1_Uca","只读","DB100.8"]
["f1Ia","Float","F1_Ia","只读","DB100.16"]
["f1Ib","Float","F1_Ib","只读","DB100.20"]
["f1Ic","Float","F1_Ic","只读","DB100.24"]
["f1P","Float","F1_P","只读","DB100.32"]
["f1Q","Float","F1_Q","只读","DB100.36"]
["f1Cos","Float","F1_COS","只读","DB100.40"]
["f1EntryPress","Float","F1_入口压力","只读","DB100.360"]
["f1ImpellerPress","Float","F1_叶轮压力","只读","DB100.364"]
["f1OutletPress","Float","F1_出口压力","只读","DB100.368"]
["f1HydraulicPress","Float","F1_液压站油压","只读","DB100.372"]
["f1StallDiffPress","Float","F1_失速压差","只读","DB100.376"]
["f1EntryTemp","Float","F1_入口温度","只读","DB100.524"]
["f1BladeMechAngle","Float","F1_叶片机械角度","只读","DB100.416"]
["f1BladeAngle","Float","F1_叶片角度","只读","DB100.412"]
["f1BladeAngleSet","Float","F1_叶片角度设定","读写","DB100.60"]
["f1FixedAngleSet","Float","F1_固定角度设定","读写","DB100.68"]
["f1StallMin","Float","F1_失速分","只读","DB100.244"]
["f1StallSec","Float","F1_失速秒","只读","DB100.248"]
["f1RunningDays","Float","F1_运行天","只读","DB100.164"]
["f1FanRunTime","Float","F1_风机运行时","只读","DB100.168"]
["f1FanRunMin","Float","F1_风机运行分","只读","DB100.172"]
["f1FanRunSec","Float","F1_风机运行秒","只读","DB100.176"]
["f1FanRunHoursAcc","Float","F1_风机运行小时累计","只读","DB101.268"]
["f1TestDamperOpen","Float","F1_测试风门开度","只读","DB100.344"]
["f1FanDamperOpen","Float","F1_风机风门开度","只读","DB100.348"]
["f1LubOilTemp","Float","F1_润滑油温","只读","DB100.488"]
["f1LubPipeTemp","Float","F1_润滑管温","只读","DB100.484"]
["f1HydraulicOilTemp","Float","F1_液压油温","只读","DB100.480"]
["f1FanACBTemp1","Float","F1_风机角接触轴承温度1","只读","DB100.456"]
["f1FanACBTemp2","Float","F1_风机角接触轴承温度2","只读","DB100.460"]
["f1FanDGBearingTemp1","Float","F1_风机深沟轴承温度1","只读","DB100.464"]
["f1FanDGBearingTemp2","Float","F1_风机深沟轴承温度2","只读","DB100.468"]
["f1FanRBearingTemp1","Float","F1_风机滚柱轴承温度1","只读","DB100.472"]
["f1FanRBearingTemp2","Float","F1_风机滚柱轴承温度2","只读","DB100.476"]
["f1MotorUTemp","Float","F1_电机U绕组温度","只读","DB100.500"]
["f1MotorVTemp","Float","F1_电机V绕组温度","只读","DB100.508"]
["f1MotorWTemp","Float","F1_电机W绕组温度","只读","DB100.516"]
["f1MotorNonDriveTemp","Float","F1_电机非驱动侧温度","只读","DB100.496"]
["f1MotorDriveTemp","Float","F1_电机驱动侧温度","只读","DB100.492"]
["f1InverterCurr","Float","F1_变频器电流","只读","DB100.424"]
["f1FreqFeedback","Float","F1_频率反馈","只读","DB100.420"]
["f1FreqSetting","Float","F1_频率设定","读写","DB100.80"]
["f1FixedFreqSetting","Float","F1_固定频率设定","读写","DB100.76"]
["f1FanVertVib","Float","F1_风机垂直振动","只读","DB100.388"]
["f1FanHorizVib","Float","F1_风机水平振动","只读","DB100.384"]
["f1AirVolume","Float","F1_风量","只读","DB100.812"]
["f2Uab","Float","F2_Uab","只读","DB200.0"]
["f2Ubc","Float","F2_Ubc","只读","DB200.4"]
["f2Uca","Float","F2_Uca","只读","DB200.8"]
["f2Ia","Float","F2_Ia","只读","DB200.16"]
["f2Ib","Float","F2_Ib","只读","DB200.20"]
["f2Ic","Float","F2_Ic","只读","DB200.24"]
["f2P","Float","F2_P","只读","DB200.32"]
["f2Q","Float","F2_Q","只读","DB200.36"]
["f2Cos","Float","F2_COS","只读","DB200.40"]
["f2EntryPress","Float","F2_入口压力","只读","DB200.360"]
["f2ImpellerPress","Float","F2_叶轮压力","只读","DB200.364"]
["f2OutletPress","Float","F2_出口压力","只读","DB200.368"]
["f2HydraulicPress","Float","F2_液压站油压","只读","DB200.372"]
["f2StallDiffPress","Float","F2_失速压差","只读","DB200.376"]
["f2EntryTemp","Float","F2_入口温度","只读","DB200.524"]
["f2BladeMechAngle","Float","F2_叶片机械角度","只读","DB200.416"]
["f2BladeAngle","Float","F2_叶片角度","只读","DB200.412"]
["f2BladeAngleSet","Float","F2_叶片角度设定","读写","DB200.60"]
["f2FixedAngleSet","Float","F2_固定角度设定","读写","DB200.68"]
["f2StallMin","Float","F2_失速分","只读","DB200.244"]
["f2StallSec","Float","F2_失速秒","只读","DB200.248"]
["f2RunningDays","Float","F2_运行天","只读","DB200.164"]
["f2FanRunTime","Float","F2_风机运行时","只读","DB200.168"]
["f2FanRunMin","Float","F2_风机运行分","只读","DB200.172"]
["f2FanRunSec","Float","F2_风机运行秒","只读","DB200.176"]
["f2FanRunHoursAcc","Float","F2_风机运行小时累计","只读","DB201.268"]
["f2TestDamperOpen","Float","F2_测试风门开度","只读","DB200.344"]
["f2FanDamperOpen","Float","F2_风机风门开度","只读","DB200.348"]
["f2LubOilTemp","Float","F2_润滑油温","只读","DB200.488"]
["f2LubPipeTemp","Float","F2_润滑管温","只读","DB200.484"]
["f2HydraulicOilTemp","Float","F2_液压油温","只读","DB200.480"]
["f2FanACBTemp1","Float","F2_风机角接触轴承温度1","只读","DB200.456"]
["f2FanACBTemp2","Float","F2_风机角接触轴承温度2","只读","DB200.460"]
["f2FanDGBearingTemp1","Float","F2_风机深沟轴承温度1","只读","DB200.464"]
["f2FanDGBearingTemp2","Float","F2_风机深沟轴承温度2","只读","DB200.468"]
["f2FanRBearingTemp1","Float","F2_风机滚柱轴承温度1","只读","DB200.472"]
["f2FanRBearingTemp2","Float","F2_风机滚柱轴承温度2","只读","DB200.476"]
["f2MotorUTemp","Float","F2_电机U绕组温度","只读","DB200.500"]
["f2MotorVTemp","Float","F2_电机V绕组温度","只读","DB200.508"]
["f2MotorWTemp","Float","F2_电机W绕组温度","只读","DB200.516"]
["f2MotorNonDriveTemp","Float","F2_电机非驱动侧温度","只读","DB200.496"]
["f2MotorDriveTemp","Float","F2_电机驱动侧温度","只读","DB200.492"]
["f2InverterCurr","Float","F2_变频器电流","只读","DB200.424"]
["f2FreqFeedback","Float","F2_频率反馈","只读","DB200.420"]
["f2FreqSetting","Float","F2_频率设定","读写","DB200.80"]
["f2FixedFreqSetting","Float","F2_固定频率设定","读写","DB200.76"]
["f2FanVertVib","Float","F2_风机垂直振动","只读","DB200.388"]
["f2FanHorizVib","Float","F2_风机水平振动","只读","DB200.384"]
["f2AirVolume","Float","F2_风量","只读","DB200.812"]
["f1ScreenStart","Boolean","F1_画面启动","只写","M1008.0"]
["f1ScreenStop","Boolean","F1_画面停止","只写","M1008.1"]
["f1ScreenAlarmClear","Boolean","F1_画面消警","只写","M1008.2"]
["f1ScreenReset","Boolean","F1_画面复位","只写","M1008.3"]
["f2ScreenStart","Boolean","F2_画面启动","只写","M2008.0"]
["f2ScreenStop","Boolean","F2_画面停止","只写","M2008.1"]
["f2ScreenAlarmClear","Boolean","F2_画面消警","只写","M2008.2"]
["f2ScreenReset","Boolean","F2_画面复位","只写","M2008.3"]